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GENERAL FEATURES
The BRP is a coil voltage regulation module designed with flexible options to prevent brake/regulator coils from being continuously exposed to high current
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1.1 [bookmark: _Toc226288292]Input Supply

	Özellik
	Açıklama 

	Supply Voltage
	220VAC
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1.2 [bookmark: _Toc226288293]Output Options
	Anahtar 1
	Anahtar 2 
	Açıklama 

	220V
	%100
	Output starts and continues at 220V

	220V
	%75
	Output starts at 220V, drops to 170V after 3 seconds

	220V
	%50
	Output starts at 220V, drops to 110V after 3 seconds

	220V
	%25
	Output starts at 220V, drops to 55V after 3 seconds

	110V
	%100
	Output starts and continues at 110V

	110V
	%75
	Output starts at 110V, drops to 75V after 3 seconds

	110V
	%50
	Output starts at 110V, drops to 55V after 3 seconds

	110V
	%25
	Output starts at 110V, drops to 35V after 3 seconds
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	Rumuz
	Açıklama 

	AC
	220 VAC Input

	AC
	220 VAC Input

	-
	Output Negative Terminal

	+
	Output Positive Terminal
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